Non Destructive Test

* 1 magnetic particle testing line
  + Magnaflux Corporation - Wet horizontal unit
  + Model H710 Full Wave DC with a 20 inch diameter
  + 5 turn coil with a Magnaflux demagnetizing unit
  + 19 inch opening, model SB-1619
  + Alternating Current, for the wet continuous method
  + Operated by Level III Technician
* 2 Fluorescent Penetrant Inspection Lines
  + One for ground support equipment and one for flight hardware and chemical process support
  + Both lines capable of Type 1 method A water wash
  + Both lines have Visible die capabilities
  + Phoenix Hand Held smart LED UV Lamp PX-45C Pro
* Both Lines are NADCAP Certified