Non Destructive Test

* 1 magnetic particle testing line
	+ Magnaflux Corporation - Wet horizontal unit
	+ Model H710 Full Wave DC with a 20 inch diameter
	+ 5 turn coil with a Magnaflux demagnetizing unit
	+ 19 inch opening, model SB-1619
	+ Alternating Current, for the wet continuous method
	+ Operated by Level III Technician
* 2 Fluorescent Penetrant Inspection Lines
	+ One for ground support equipment and one for flight hardware and chemical process support
	+ Both lines capable of Type 1 method A water wash
	+ Both lines have Visible die capabilities
	+ Phoenix Hand Held smart LED UV Lamp PX-45C Pro
* Both Lines are NADCAP Certified