**Seyer Industries – Chemical Processing Capabilities**

Seyer Industries is committed to providing our customers with top tier delivery and quality. In efforts to become more vertically integrated, Seyer has installed a state-of-the-art metal finishing line to its core capabilities. Below is a list of specifications and processes Seyer will be able to provide:

* **Anodize**
  + MIL-A-8625
    - Type IC – Boric Sulfuric
    - Type IIB – Thin Film
* **Conversion Coat**
  + MIL-DTL-5541
    - Class IA
* **Passivation**
  + SAE-AMS-2700
    - Type II
    - Type VI
  + ASTM A 967
    - Type II
    - Type VI
* **Pre-Penetrant Etch**
  + ASTM E 1417
  + Per Prime / Customer Specification
* **Aluminum Etch**
  + Per Prime / Customer Specification
* **Titanium Etch**
  + Per Prime / Customer Specification
* **Tank Size**
  + Tank Size: 33” Wide x 60” Long x 60” Deep
  + Tank Volume: 542 gallons